/etc/ltsp/dhcpd.conf

#
# Default LTSP dhcpd.conf config file.
#
authoritative;
subnet 192.168.10.0 netmask 255.255.255.0 {
# range 192.168.10.201 192.168.10.210;
option domain-name "intracentre";
option domain-name-servers 192.168.0.1;
option broadcast-address 192.168.10.255;
option routers 192.168.10.7;
# next-server 192.168.0.8;
# get-lease-hostnames true;
option subnet-mask 255.255.255.0;
option root-path "/opt/ltsp/i386";
if substring( option vendor-class-identifier, 0, 9 ) = "PXEClient" {
filename "/ltsp/i386/pxelinux.0";
} else {
filename "/ltsp/i386/nbi.img";
}
}
###
# Aula d'informàtica de la primera planta
###
host aula1 {
hardware ethernet 00:0b:cd:48:09:47;
fixed-address 192.168.10.101;
}
host aula2 {
hardware ethernet 00:0b:cd:dd:85:c8;
fixed-address 192.168.10.102;
}
host aula3 {
hardware ethernet 00:0b:cd:66:aa:dc;
fixed-address 192.168.10.103;
}
host aula4 {
hardware ethernet 00:0b:cd:63:eb:83;
fixed-address 192.168.10.104;
}
host aula5 {
hardware ethernet 00:0b:cd:c3:3a:cb;
fixed-address 192.168.10.105;
}
host aula6 {
hardware ethernet 00:0b:cd:a0:0c:6f;
fixed-address 192.168.10.106;
}
host aula7 {
hardware ethernet 00:0b:cd:64:a0:ce;
fixed-address 192.168.10.107;
}
host aula8 {
hardware ethernet 00:0b:cd:e0:ee:82;
fixed-address 192.168.10.108;
}
host aula9 {
hardware ethernet 00:0b:cd:63:37:a9;
fixed-address 192.168.10.109;
}
host aula10 {
hardware ethernet 00:0b:cd:c3:3a:d0;
fixed-address 192.168.10.110;
}
host aula11 {
hardware ethernet 00:0b:cd:49:fd:78;
fixed-address 192.168.10.111;
}
host aula12 {
hardware ethernet 00:0b:cd:c3:3a:d1;
fixed-address 192.168.10.112;
}
host aula13 {
hardware ethernet 00:0b:cd:63:11:b2;
fixed-address 192.168.10.113;
}
host aula14 {
hardware ethernet 00:0b:cd:64:cf:54;
fixed-address 192.168.10.114;
}

Inici de l'Espai | Menú de Documents | Servidors LTSP | Implementació de LINUX/UBUNTU